350 Series

Furnish and install 350 Series Model___________ baseboard cover assembly as manufactured by Slant/Fin Corporation, consisting of one-piece bottom, back and top panel, and one-piece 19 (16) gauge front panel, formed of cold rolled steel. Bottom and top edges of back panel shall be formed to provide channels along entire length, to receive full-height support brackets.

Brackets shall be die formed of electro-galvanized cold rolled steel, for rigid bracing and spring locking. Slide-action expansion cradles, formed of polypropylene, shall be inserted between heating element and support bracket. Cradles shall protect element bottom and sides from contact with brackets or cover, confining element to free lateral expansion for noiseless operation.

Provide all required accessories for a complete installation. Cover accessories shall be telescopic and shall match enclosure color. All cover components shall be painted in Nu White, oven baked melamine cross-linked polyester enamel.

